1. Instal IP-clamp 1.2, *DO NOT REBOOT* and *DO NOT EXECUTE IT*!


2. Fire our keygen, press Crack and pick Cebas/Ip-clamp dir.
 (only the public crypto key will be patched)


3. Now you can reboot and make sure ipclamp service is running.


4. Launch IP-Clamp.exe and choose 'localhost' as primary network adapter, apply.

5. Create a request file using your personnal informations
 and a licence code generated by our keygen.


6. Use keygen to generate a valid licence ipclamp.lic from this request.
 Save the lic where except in IPClamp's dir (otherwise you won't
   be able to import the it).


7. Import your licence in IP-Clamp.


8. Install every Cebas plug-ins you need.

9. Enjoy it!


